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The Performing Arts Center, SUNY Purchase



The Concert Hall
Technical Packet











The Performing Arts Center is a full service performance facility.  The Performing Arts Center maintains a central inventory of equipment for most theatrical and concert needs.  Due to the nature of the facility as a four Theater complex we do not publish inventory lists.  To ensure that the needs of your production are met we request that you communicate your requirements to us as soon as possible, so that we can make the appropriate allocations.  You will find, listed by department, the general types of equipment that we carry.  For further information please feel free to contact the Production Office.

Vectorworks and PDF files of the theater’s ground plan and section, as well as lineset schedule, are available by request. 

The Performing Arts Center's address is

Mailing:
The Performing Arts Center,
SUNY Purchase
ATTN: Production Office
735 Anderson Hill Rd.
Purchase, NY  10577

For Shipping to loading docks:
	Please contact the Director of Production for specific instructions (914) 251-6266 

Performing Arts Center Contact List:

Megan Corkrum 			(914) 251-6266
Director of Production		megan.corkrum@Purchase.edu

Peter Specce,			(914) 251-6221
Asst. Director of Production		Peter.Specce@Purchase.edu

Justin Herminghouse		(914) 251-6240
Production Technolgy Manager 		Justin.Herminghouse@Purchase.edu

Bennett Marrow			(914) 251-6219
Production Coordinator		Bennett.Marrow@Purchase.edu


Seating Capacity:
Orchestra	732
Grand Tier	232
Balcony	336
	1300

Pit rows (removable)	72
	1372

THE CONCERT HALL STAGING:   
Loading Dock Access:

The Concert Hall has two loading docks, the primary one accessed through Parking Lot West 1.  Both are truck level, and can handle one 53' tractor-trailer each.  Dock height is 4’-0”.  Stage right in West 1 is a blind side back in.  Stage left, via the paint shop in parking lot West 2, is a left hand back in, and is available by prior arrangement only. Trucks may not park in the loading docks.  Overnight parking for trucks is available by prior arrangement in Parking Lot West 2.  During the winter months, trucks are not permitted to idle in the loading docks due to the location of the air intakes for the building.


Stage Deck, Stage Lifts, Flooring:

The stage deck is a semi-sprung floor with a Stagelam phenolic resin covering.  Due to the nature of this material, lagging and screwing are prohibited. 
The Concert Hall is equipped with 2 full stage lifts downstage of the proscenium.  Normally the downstage lift holds two rows of removable seating, and the upstage lift plays at stage level as an extended apron.  There is no seating available for the upstage lift.  For loading in/out and adjusting orchestra pit levels, the lifts can operate independently, but must remain stationary during performances.
The Theater has a Harlequin dance floor.  There is enough flooring to cover the playing depth of our Theater upstage of the proscenium.  The floor is black and grey reversible floor. A white Marely floor is available with previous arrangements 

The Center does NOT have a forklift. You will need to rent one if needed. 

Rigging:

The Theater is equipped with a single purchase counterweight system.  Arbor capacity is 1200 lbs. above batten weight.  The length of each batten is 60'.  There are 4' batten extensions in limited availability.  There are 66 linesets in this Theater, 3 of them are dedicated to carrying ceiling pieces for the orchestra shell.  Our current lineset schedule is available upon request.  

Labor:

The stagehands at the Performing Arts Center are professional, free lance, union stagehands and wardrobe personnel. We abide by many standard union labor rules. For shows traveling with a “Yellow-Card" we are under the jurisdiction of the New York City and Westchester IATSE Local 1. If you are unfamiliar with the area please contact the Production Office and we will help you arrange your labor through the local Business Office.

General Equipment:

Each theater is equipped with a variety of A-frame ladders and a personnel Genie lift.

The PERFORMING ARTS CENTER owns orchestra chairs, bass stools, music stands and lights for orchestra use.  There are 4' x 8' risers in heights of 8", 16" and 24".  We do not own choral risers.  The Concert Hall also houses an acoustical concert shell which is available by prior arrangement.  It has a variety of possible configurations depending on orchestra size.

The Performing Arts Center maintains a wide assortment of concert quality Steinway pianos which are available by prior arrangement.  Please be advised that THE PERFORMING ARTS CENTER DOES NOT ALLOW TAPE OR ADHESIVES OF ANY KIND ON ANY OF THE PIANOS OR PREPARED PIANO. THERE ARE NO EXCEPTIONS TO THIS POLICY AND WILL BE STRICLTLY ENFORCED.

The PERFORMING ARTS CENTER has a Steinway-trained house piano tuner, contact the production office in advance to arrange tunings, standbys and to discuss associated fees.

The house maintains a lecture package including a lectern, chairs, and tables with appropriate skirting, available on request.  

Organ Room:

The Organ Room, which is located stage right adjacent to the Theater, it can be used as a rehearsal room by prior request. Maximum occupancy is 49.

The available floor space is approximately 55' x 41'.  The floor is maple tongue and groove and there are mirrors and dance bars to accommodate dance rehearsals.  The PERFORMING ARTS CENTER can also supply a dance floor for this area, available through prior arrangement. No screws, lags, or nails are permitted in this floor at any time. There are no exceptions to this policy. 

Flentrop Organ:

The Theater has, normally in storage, a large, movable, tracker organ.  The organ can be moved onto the Concert Hall Stage for performances, through prior arrangement.
The organ was built by Flentrop in 1966 and has 61 ranks.  For additional information and specifications, please contact the Production Office.









Dressing Rooms:

Dressing rooms for this Theater are located one floor below stage level and are accessible via the stairs stage right and stage left or via freight elevator located in the adjacent paint deck.  All rooms have makeup mirrors and lights, tables and chairs.  There are restroom facilities and showers located in each dressing room.  Dressing Rooms break down is as follows:
		4 chorus rooms		10-15 people each
		10 private rooms		2 people each
Laundry:
There are shared laundry facilities located in an adjacent section of the building which must be reserved for use in advance of load-in.  We can supply washing, drying and ironing facilities. Portable steamers are available through prior arrangement.




Special Effects:

Any special effects, including but not limited to Fog, Haze, Confetti, Pyrotechnics, must be approved by the Production Office prior to load in.  All necessary and appropriate certificates must be presented upon arrival.

Wireless Internet

There is Wi-Fi available on the stage, wings, house, dressing rooms, and the lobby. 

Wired Internet

There is a wired internet connection in the center booth on the orchestra level used for livestream. 


For Visiting Wireless Access: 
Network: Purchase Guest
Password: (Please Ask Production Staff Member)












The Concert Hall Dimensions
Loading Dock Doors SR:		9'-9"h x 7'-9"w    	2.97m x 2.36m
Loading Dock Doors SL		10'-0"h x 12'-0"w	3.05m x 3.66m
Dock Height SL & SR:		4’-0"		     	1.22m
Control Booth to Plaster Line:	82'-0"		   	25m
Follow Spot Booth to Plaster Line:	85'-0"			25.91m
2nd Bridge to Plaster Line:		85'-0"			25.91m
1st  Bridge to Plaster Line:		60'-0"			18.29m
FOH Balc Rail to Plaster Line:	61'0"			18.59m
Proscenium Width:			53'-10 1/2"	 	16.42m
Proscenium Height: 			36'-0"		 	10.97m
Total Playing Depth:			73'-7"			22.43m
  	 (US lift incld.)
Stage Depth:				54'-9"			16.69m		
	(Plaster line to back wall)
Stage Lifts at Centerline:
	Downstage-depth:		6'-8"		   	2.03m
	Upstage-depth:		11'-10"		   	3.60m
Apron at Centerline Depth:		7'-0"		   	2.13m
Stage Height from House Floor	3’-1”			0.94m
Stage Left Wing:  			24'-6"		   	7.46m
Stage Right Wing:  			58'-6"		 	17.83m
Grid Height:				83'8"		 	25.50m
High Steel:				90'8"		 	27.63m
Batten Working Height:       		4'-0"		 	1.9m
Batten Working Weight:  		1200 lbs.	   	589.67kg
Batten Length:				60'-0"		 	18.28m
Batten Extension			4'-0"			1.22m
Masking Opening:			45'0"		 	13.72m
Lighting Angles:
	Approximate measurements from hanging position to plaster line, center stage
First Bridge						48°
Second Bridge	/Follow Spot Booth			31°

The Concert Hall Drapery Inventory:
Black Legs			12		15'w x 40'h		4.57m x 12.19m
Black Border			3		60'w x 20'h		18.29m x 6.10m
Black Border			4		60'w x 15'h		18.29m x 4.57m
Blackout Cloth		2		60'w x 40'h		18.29m x 12.19m
Tab Curtains			4		6'w x 40'h		1.83m x 12.19m
Half-Traveler			2		34'w x 40'h		10.36m x 12.19m
Black Scrim			1		56'w x 45'h		19.81m x 13.72m
White Bounce			1		65'w x 45'h		19.81m x 13.72m
Rear Projection Screen	1		60’w x 40’h		18.29m x 12.19m
Movie Screen			1		40’w x 20’h		18.29m x 6.10m 
Main Curtain (red velour)	1		60’w x 40’h		18.29m x 12.19m


The Concert Hall Lighting and Electrical Information:

Control: 

The Concert Hall is equipped with an ETC Ion 6K, 2x20 Fader Wing, (2) Touchscreen Monitors.  An ETC Net3 RVI with 2 flat screen monitors available. An Ipad with Remote App is available on request as the remote for this console. The control booth is located at the rear of the Grand Tier.  

DMX In ports are available for any touring consoles which may need to access the house system.  They are located as follows:

	Control Booth
	Tech Table Position (center of the orchestra)
	Downstage Left on the Proscenium Wall

There are three DMX In ports located at each position, allowing control of the house system (DMX addresses 1-512) and 1024 additional DMX addresses.

DMX Out ports are available to add additional dimmers, scrollers, moving lights, and any other DMX-protocol equipment.  They are located as follows:

	FOH - 1st Bridge, SL and SR
	Midrail - SL and SR
		Stage level - DSL, DSR, and USL.  

The Concert Hall is equipped with a Lighting Control Network. Using ACN and sACN protocol for control of Dimmers and DMX Out ports. Ethernet Ports are located in the Lighting Booth, Tech Table, SL/SR Deck and Dimmer room. 

Company Power:

There are two 400 amp three phase, 208v disconnects in the stage area, distributed as follows:
	
	1)  USL on the stage level with Camlock connections
	2)  USR or USL at the mid-rail with Camlock connections (parallel service)
		Services NOT ground & neutral reversed.

In addition, there are four 400A, 208v company switches available in the dimmer room. These four disconnects draw from the same power that feeds the theater’s dimming system. The combined load on the company switches plus the house system cannot exceed 1500 amps/phase.  These disconnects are equipped with cam-lock connectors which are NOT ground & neutral reversed. 






House Dimmers and Circuitry:

The Concert Hall has 558 ETC dimmers (dimmer-per-circuit), configured as follows:
	
The house circuitry consists of 20A (to 2.4 Kw dimmers) and 50A (to 6.0 Kw dimmers) 2P&G (stage pin) connectors.  If you anticipate using any 50 amp circuits, please check with the Lighting Supervisor for availability of 50A cable. 

House Lights:

House lights are dimmable from the control booth, and from downstage left and downstage right.  House lights may also be controlled through the control console, or any touring console with DMX protocol. 

House Hang:

There is a permanent Front of House hang. Overhead are four linesets hung with strip lights without color, predominantly used for worklight and general illumination. These strip lights can be used or struck as needed. There are an additional 3 linesets with installed electrical raceways, and there are 5 additional pairs of dropboxes which may be moved to any lineset needed.

Follow Spots:

The theater has 2 Lycian StarkLite II 1.2kw follow spots located in a spot booth at the back of the house in the center of the 2nd bridge above the balcony seating.





















The Concert Hall Audio:

Auditorium Amplification

The Concert Hall has a two channel house speaker system as well as a delay fill system for the balcony. The PA System is composed of  (18) QSC  LA 108. Two flown arrays with (9) 8” two-way active line array loudspeakers on each side. There are two permeant subwoofer positions on the deck on the house right and house left of the proscenium. They are composed of  (6) QSC - L118 18” direct-radiating actrive subwoofers on each side. The signal for the PA system also feeds three digital delay aligned, hung from the rear of the first lighting bridge, which provide improved intelligibility for the balcony seats.  

House Audio Console

The house console is a Yamaha DM7.

Additional House Equipment

In addition to the console, the house system is also equipped with two Denon DN-C501 (CD / USB / iPod) players, interfaced to the console via the house Dante network. 

This theater is also equipped with a computer dedicated to audio with a variety of software including Show Cue System, Stage Research SFX 6.1, Yamaha QL Editor and Studio Manager, Shure Wireless Workbench, Wavelab 7, Reaper, etc. Audio is interfaced via Dante Virtual Soundcard. The computer does not provide internet access.

The console and associated electronics are located in the control booth at the rear house left side of the Grand Tier level.

Audio Snake

The main house snake has 54 channels with parallel boxes located on the stage left and stage right proscenium walls.  Each box, as well as the control booth, also has a Ramlatch panel mount connector (wired to the Ramlatch standard).  There are six audio tie lines that run from the theater patchbay to a breakout box in the booth at the rear center of the Orchestra level. Additional speaker lines and mic jacks are located throughout the house and stage areas.  There are twelve audio tie lines running from the Theater’s patch bay to a central patch point for the facility that can be used to cross-connect audio from various spaces within the facility. 

Audio Power

There are two 20 amp AC lines running from the control booth to the stage right proscenium wall that can be used to feed power from the booth circuit panel to equipment located backstage.  The AC lines are terminated with L5-20 connectors, with 5-20 (“Edison”) adapters available.

Audio Rigging

The theater is also equipped with certified rigging points and 3 installed 1-ton chain motors on a reverse “L” shaped truss for the hanging of a stereo speaker system located at stage right and left proscenium. Please Note: The Performing Arts center does not currently own any type of flown speaker system. 

Communication:

The Concert Hall is equipped with a single channel Clear Com system which is accessible from virtually all points within the Theater.  There is also a house page/monitor system which puts program feed to the booths and dressing rooms. Six headsets and belt packs are included in the venue’s basic audio package.


Additional Audio Equipment:

The Performing Arts Center maintains an extensive inventory of playback equipment, microphones, speakers, amplifiers, signal processing equipment, additional intercom equipment, cables, and accessories. Rental charges may apply. Due to the constant rotation of our inventory among our theaters, we are unable to publish equipment lists. Please feel free to call the Production Office and speak with either the Director of Production or Audio Supervisor regarding the specific needs of your production.
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