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The Performing Arts Center. SUNY Purchase



The PepsiCo Theater
Technical Packet



The Performing Arts Center is a full service performance facility.  The Performing Arts Center maintains a central inventory of equipment for most theatrical and concert needs.  Due to the nature of the facility as a four Theater complex we do not publish inventory lists.  To ensure that the needs of your production are met we request that you communicate your requirements to us as soon as possible, so that we can make the appropriate allocations.  You will find, listed by department, the general types of equipment that we carry.  For further information please feel free to contact the Production Office.

Vectorworks and PDF files of the theater’s ground plan and section, as well as lineset schedule, are available by request. 

For further inquiries about space or equipment availability, please contact the Director of Production at (914) 251-6266 or megan.corkrum@purchase.edu. 


The Performing Arts Center's address is

Mailing:
Performing Arts Center,
Purchase College 
ATTN: Production Office
735 Anderson Hill Rd.		
            Purchase, NY  10577

For Shipping to loading docks:
	Please contact the Director of Production for specific instructions (914) 251-6266 



		

For visiting wireless access: 
Log in: Purchase Guest
Password: (Please Ask Production Staff Member) 

PEPSICO THEATER STAGING:
Loading Dock Access:

The PepsiCo Theater has one loading dock, accessed through Parking Lot West 1.  It is truck level, can handle one 53’ tractor trailer at a time. Dock height is 4’-0”.  Overnight parking for trucks is available by prior arrangement in Parking Lot West 2.

Stage Deck, Stage Lifts, Flooring:

The PepsiCo Theater is equipped with 2 full stage lifts downstage of the proscenium.  Normally both lifts hold five rows (total) of removable seating.  For loading in/out and adjusting orchestra pit levels, the lifts can operate independently and, but must remain stationary during performances.  The Hanamichi platforms in the house extend over both the US and DS lifts.  In order for both the US or DS lift to become flush with the stage, the edges of the lift must remain completely clear of any materials. Drilling or lagging into the floor is strictly prohibited.

The PepsiCo Theater has a Harlequin dance floor.  The floor has been cut to 45’.  There is enough flooring to cover the playing depth of our Theater upstage of the proscenium.  The floor is a black and grey reversible floor. A white Marley floor is available with previous arrangements

	The Center does NOT have a forklift. You will need to rent one if needed  

Rigging:

The Theater is equipped with a single purchase counterweight system.  Arbor capacity is 1,200 lbs. above batten weight.  All battens are 60’ in length with limited 4’ extensions available.  There are 74 linesets available for variable use in The PepsiCo Theater.  Our current lineset schedule is available upon request.  The house curtain is blue and a guillotine type, operated from the deck, stage right.  There is a center split, but it does not travel.

Labor:

The stagehands at the Performing Arts Center are professional, free lance, union stagehands and wardrobe personnel. We abide by many standard union labor rules. For shows traveling with a “Yellow-Card" we are under the jurisdiction of the New York City and Westchester IATSE Local 1. If you are unfamiliar with the area please contact the Production Office and we will help you arrange your labor through the local Business Office.

General Equipment:

Each theater is equipped with a variety of A-frame ladders and a personnel lift.

The Performing Arts Center owns orchestral chairs, bass stools, music stands, and lights for orchestra use.  There are 4’ x 8’ risers in heights of 8”, 16” and 24”.  We do not own choral risers.  

The PERFORMING ARTS CENTER also maintains an assortment of concert quality Steinway pianos which are available by prior arrangement.  Please be advised that THE PERFORMING ARTS CENTER DOES NOT ALLOW TAPE OR ADHESIVES OF ANY KIND ON ANY OF THE PIANO OR PREPARED PIANO. THERE ARE NO EXCEPTIONS TO THIS POLICY AND WILL BE STRICLTLY ENFORCED.

The PERFORMING ARTS CENTER has a Steinway trained house piano tuner, contact the production office in advance to arrange tunings, standbys and to discuss associated fees.

The house also maintains a lecture package including a lectern, chairs, and tables, and front projection movie screen available through prior arrangement.

Dressing Rooms:

Dressing rooms for this Theater are located one floor below stage level, and accessible via stairs stage right and stage left or by the freight elevator, located stage left. All have makeup mirrors and lights, with tables and chairs.  There are restroom facilities and showers located in each dressing room.  Rooms breakdown as follows:

		4 chorus rooms		10-15 people each.
		6 private rooms		2 people each.

Laundry:

There are shared laundry facilities located in an adjacent section of the building which must be reserved for use in advance of load-in.  We can supply washing, drying and ironing facilities.  Portable steamers are available through prior arrangement.













Projection:

Panasonic PTDZ21K Projector (21,000 lumens) with option of LE20 or LE30 lenses
The projector is permanently located in the center tech booth in the back of the orchestra level The system includes a Crestron Touch Controller with multiple inputs, and an Oppo HD BluRay player.
There are ports to plug in sources at the Booth and at the House Mix position as well as on the Proscenium wall stage right for both HDMI and VGA which are configured to accept sound for playback as well.

The projectors normal focus is 18' tall x 36' wide image on our in house perforated front projection screen that is approximately 22' tall by 46' wide and is permanently located on line set #8, located approximately 5’4” upstage of the proscenium wall. Various borders and wings can adjust final image size. It is also possible to project on an upstage cyc or onto scenic elements.

Seating Capacity:

	Orchestra		 405
	Balcony		 197
	Pit   rows		   71
	Lift rows		   40
			Total:    713

Special Effects:

Any special or pyrotechnic effects must be approved by the production office prior to load in.  All necessary and appropriate certificates must be presented upon arrival.

Wireless Internet

There is Wi-Fi available on the stage, wings, house, dressing rooms, and the lobby. 


For visiting wireless access: 
Log in: Purchase Guest
Password: (Please Ask Production Staff Member)


PepsiCo Theater Dimensions

Loading Dock Doors:	9’-9”h x 7’-9”w 			2.97m x 2.36m
Dock Height:	4’-0”				1.22m
Control Booth to Plaster Line:	78’-9”				24m
2nd Bridge to Plaster Line:	75'-0"				22.86m
1st  Bridge to Plaster Line:	35'-6"				10.82m
FOH Balc Rail to Plaster Line		51’-7”				15.72m
Proscenium Width:	54’-9”				16.69m
Proscenium Height: 	28’-0”				8.53m
Total Playing Depth:	48'-9"				14.86m
	(Apron incld.)
Stage depth:	43’-10”				13.36m
	(Plaster line to back wall)
Stage Lifts at Centerline:
  	Downstage-depth:		8'-7"				2.62m   CURRENTLY HAS SEATS
	Upstage-depth:			9’-7”				2.92m   CURRENTLY HAS SEATS
Apron at Centerline Depth:	7’-7”				2.31m
Stage Height from House Floor	3’-1”				0.94m
Stage left wing:    	21’-7”				6.58m
Stage right wing:	18’-10”				5.74m
Grid Height:				75'-0"				22.86m
High Steel:				82'-3"				25.07m
Batten working height:	4'-6"				1.37m
Batten working weight:	1200 lbs.			544.3kg
Batten length:	60’-0”				18.29m
Batten Extension:	4'-0"				1.22m
Masking opening:	40’-0”				12.19m
Projection Bay:				37'-0"w x 37'-0"d		11.28m x 11.28m

The PepsiCo Theater Drapery Inventory:

Black Legs	10		15’w x 35’h	4.57m x 10.67m
Black Borders	4	60’w x 12’h			18.29m x 3.66m
Black Borders	2	60’w x 15’h			18.29m x 4.57m
Blackout Cloths	2	60’w x 35’h	18.29m x 10.67m
Tab Curtains	4	6’w x 35’h	1.83m x 10.67m
Half-Travelers	2	34’w x 35’h	10.36m x 10.67m
Black Scrim	1	65’w x 40’h	19.81m x 12.19m
White Seamless Cyc	1	65’w x 40’h	19.81m x 12.19m
Movie Screen	1	48'-6"w x 22'-0"h	14.78m x 6.71m
Main Curtain		1		60’w x 40’h			18.29m x 12.19m









The PepsiCo Theater Lighting and Electrical

Control: 

The PepsiCo Theater is equipped with an ETC IonXE with 1x touch screen monitor and 1x flat screen monitor, 2x20 Fader Wing.  An ETC Net3 RVI with 2 flat screen monitors available on request. An Ipad with iRFR app is available on request as the remote for the console.  The control booth is located at the rear of the orchestra level.

The PepsiCo is equipped with a Lighting Control Network. Using ACN and sACN protocol for control of Dimmers and DMX Out ports. Ethernet Ports are located in the Lighting Booth, Tech Table, SL/SR Deck, Dimmer room and other locations. 

DMX In ports are available for any touring consoles which may need to access the house system.  They are located as follows:

	Control booth
	Tech table position (center orchestra)
	Downstage left
	Downstage right

There are two DMX In ports located at each position, allowing control of the house system (DMX addresses 1-439).

DMX Out ports are available to add additional dimmers, scrollers, moving lights, and any other DMX-addressable equipment.  They are located as follows:

	FOH - 1st Bridge, SL and SR
	Midrail - SL and SR
		Stage level - DSL and DSR
		Other Locations now available over Network/Gateway.

Company Power:

There are three (3) 400A, 208v company switches available in the dimmer room. These three disconnects draw from the same power that feeds the theater’s dimming system. The combined load on the company switches plus the house system cannot exceed 1200 amps/phase.  These disconnects are equipped with cam-lock connectors which are NOT ground & neutral reversed. 

There is one 400 amp/three phase, 208v disconnect in the stage area which may be tapped from either USL or USR at midrail.  These disconnects are equipped with Camlock Tails NOT ground & neutral reversed.





House Dimmers and Circuitry:

The PepsiCo Theater has 412 ETC dimmers (dimmer-per-circuit), configured as follows:

	Circuit		Dimmer	Capacity
	1-376		1-376		2.4 Kw
	501-536	377-412	6.0 Kw

The house circuitry consists of 20A (to 2.4 Kw dimmers) and 50A (to 6.0 Kw dimmers) 2p&g connectors.  If you anticipate using any 50 amp circuits, please check with the Lighting Supervisor for availability of 50A cable.

House Lights:

House lights are dimmable from the control booth, and from downstage left and downstage right.  House lights may also be controlled through the control console, or any touring console with DMX and sACN protocol.

House Hang:

There is a permanent Front of House hang, which is available upon request. Overhead are two (2) linesets hung with strip lights without color, predominantly used for work light and general illumination. These strip lights can be struck as needed. 

Follow Spots:

The theater has 2 Lycian StarkLite II 1.2kw follow spots located in a spot booth at the back of the house in the center of the 2nd bridge above the balcony seating.




















Additional Lighting Inventory:

The Performing Arts Center maintains a large inventory of ETC, Altman and other various instruments which is available to the user. Rental charges may apply. Due to the constant rotation of our inventory among our four theaters, we do not list fixtures quantities. Lighting equipment can be requested by completing an “Electrics Request Form”. Below is a list of a selection of fixture types in the PAC Inventory. For further information please contact the PAC Lighting Supervisor or the Production Department (914)251-6262

	Focusing Units
	Frame Size

	ETC Source Four 5o @575w
	14"x14"

	ETC Source Four 10o @575w
	12"x12"

	ETC Source Four 19o @575w
	6.25"x6.25"

	ETC Source Four 26o @575w
	6.25"x6.25"

	ETC Source Four 36o @575w
	6.25"x6.25"

	ETC Source Four 50o @575w
	6.25"x6.25"

	

	

	Wash Units
	Frames Size

	PAR 64, 1Kw
	10"x10"

	ETC S4 PAR, 750w
	7.5"x7.5"

	8" Fresnel, 1Kw
	10"x10"

	6" Fresnel, 750w
	7.5"x7.5"

	3" Fresnel, 300w
	3.75"x3.75"

	Mini-ten, 1Kw
	8.75"x5.5"

	14" Scoop, T-3, 1Kw
	14"x14"

	Birdie, 150w
	2.75"x2.75"

	GAM Stick-up, 150w
	N.F.

	
	

	

CYC and Border Lights
	

Frames Size

	FAR-CYC, T-3, 4 CKT, 4 light, 1K per CKT, Top/Bottom
	15"x18"

	 ALT T-3, 3 CKT, 6 light, 1K per CKT (Length 4'6")
	8.5"x12.75"

	KLG T-3, 3 CKT, 9 light, 1K per CKT  (Length 6'-9")
	8.5"x8.5"

	KLG T-3, 4 CKT, 8 light, 1K per CKT (Length 6')
	8.5"x8.5"

	KLG T-3 4 CKT 12 light, 1.5K per CKT (length 8')
	7.25"x7.75"




The PepsiCo Theater Audio:

Auditorium Amplification:

For front of house sound reinforcement, the PepsiCo Theater is equipped with a matching Left, Center, and right speaker arrays dead hung through cutouts in the venue’s acoustical cloud. Each array consists of two L-Acoustics ARCS Focus cabinets over two ARCS Wide cabinets. Each array is powered by an L-Acoustics LA4X amplified controller.
There are a total of four L-Acoustics SB28 subwoofers with two dead hung just off stage of either side of the acoustical cloud. The subwoofers are powered by an L-Acoustics LA12X amplified controller.
Additionally, there are a total of eight L-Acoustics 5XT fill speakers on the underside of the balcony positioned to cover the rear audience and operator booths. The fills are powered by an L-Acoustics LA4X amplified controller.

Additionally, as part of the venue’s cinema sound sound system, there are a total of ten QSC SR- 1020 surround loudspeakers. They are located symmetrically with four up each side of the orchestra and one on each side of the balcony. Each is driven individually by a dedicated channel of a QSC DPA 4.30 amplifier. By prior arrangement, the surround loudspeakers can be reassigned for use by the main sound system for effects.

Mixing Console and Inputs:

The venue’s mixing console is a Yamaha CL5. It is normally located in a booth at the rear of the orchestra level. By prior arrangement / approval it may be possible to move it out to a fixed position at the rear of the Orchestra, with an attendant loss of twenty four seats.

The console is normally fed by a Rio3224-D located backstage and connected to the house snake boxes on the proscenium walls via patch bays. There is an additional Rio1608-D located in the control booth and connected to the patch bays there.

Communication:

The PepsiCo Theater is equipped with a single channel Clear Com system which is accessible from virtually all points within the Theater. There is also a house page/monitor system which puts program feed to the booths and dressing rooms. 

Additional Audio Equipment:

The Performing Arts Center maintains an extensive inventory of playback equipment, microphones, speakers, amplifiers, signal processing equipment, additional intercom equipment, cables, and accessories. Rental charges may apply. Due to the constant rotation of our inventory among our theaters, we are unable to publish equipment lists. Please feel free to call the Production Office and speak with either the Director of Production or Audio Supervisor regarding the specific needs of your production.

Performing Arts Center Contact List:

Megan Corkrum 			(914) 251-6266
Director of Production		megan.corkrum@Purchase.edu

Peter Specce,			(914) 251-6221
Asst. Director of Production		Peter.Specce@Purchase.edu

Justin Herminghouse		(914) 251-6240
Production Technology Manager		Justin.Herminghouse@Purchase.edu

Bennett Marrow			(914) 251-6219
Production Coordinator		Bennett.Marrow@Purchase.edu


Rental Booking Manager		(914) 251-6232
Box Office – Sales/Ticket Purchases		(914) 251-6200
Box Office – Manager		(914) 251-6212

Performing Arts Center Website:		www.artscenter.org
Site contains venue information and e-mail links to most of the center's staff

DINING

[bookmark: _Hlk217146609]On-Campus Dining hours will change during school breaks
Hours Subject to Change (and quite often do change, especially around holidays) without notice.

Campus Center North/ The Hub			Starbucks 
On Purchase campus				On Purchase Campus
Mon – Fri  7:30am – 12:00am			Located in Fort Awesome
Sat – 10:00am – 1:00am			On Lincoln Ave
Sun – 10:00am- 12:00am			(914) 251-6988
					Mon-Fri 7:30am-11pm
				Sat&Sun 10am-11pm

Enstein Bagels 			 
On Purchase campus	
Located 			
Mon – Fri  7:30am – 3:00pm			
Sat & Sun – Closed	








Hospitals & Medical Info: 

White Plains Hospital				Rye Walk-in Medical Center
41 East Post Road					150 Purchase Street
White Plains, NY 10601				Rye, NY 10580 
(914) 681-0600					(914) 967-3266
www.wphospital.org 					M-F 8am-7pm
Sat 9am-2:00pm
Sun 10am-2:00pm

Stop & Shop Pharmacy				Greenwich Hospital
154 Westchester Avenue				5 Perryridge Road
White Plains, NY 10604				Greenwich, CT 06830
914-997-1530		203-863-3000
Mon-Fri: 8am-8am 		www.greenhosp.org
Sat: 9am-5pm
Sun: 9am-3pm































Directions to Purchase College, SUNY Performing Arts Center:


Location Access via:
	Parking Lot West 1
	Underpass in between 
Parking Lots West 1 and West 2
	Parking Lot West 2

	· The Concert Hall “A” Loading Dock
· PepsiCo Theater “B” Loading Dock
	· Main Lobby
· Box office
· Administrative offices
· ADA Elevator
· The Repertory Theater “D” *
Loading Area and Elevator
	· Recital Hall “C”  Loading Dock
· Paint Deck 
  (Concert Hall Alternate Loading Dock)
· ALL Overnight Parking
    (With Prior Approval)


* The Repertory Theater (“D”) does not have a dedicated Loading Dock. Loading is done on street level in the underpass, which has direct access to the stage lift and freight elevator. The Repertory Theater Stage Lift runs from the street level to stage level.

By Car:

From New York City, Southern Westchester, and Long Island:
Take the Hutchinson River Parkway, north to Exit 28, Lincoln Avenue.  Turn left onto Lincoln Avenue and proceed approximately one mile to Anderson Hill Road (2nd traffic light).  Turn right onto Anderson Hill Road.  The campus is immediately on the left.

From Rockland County and Northern New Jersey (via the Tappan Zee Bridge):
Take I-287 (Cross Westchester Expressway) to exit 8E.  Shortly after first traffic light, bear left onto Anderson Hill Road.  Proceed approximately 2.5 miles.  The campus is on the left, just after intersection at Lincoln Avenue.

From Northern Westchester:
Take I-684 south to Exit 2 (Route 120), drive over the bridge and turn right onto Route 120 South (Purchase Street).  Follow Route 120 south, 3.2 miles to Anderson Hill Road (1st traffic light) and turn left.  Take Anderson Hill Road to 2nd traffic light.  The campus is on the left, just after intersection at Lincoln Avenue.

From Connecticut, via the Merritt Parkway (which becomes the Hutchinson River Parkway in New York State):
Proceed south to the New York Exit 28, Lincoln Avenue (Note: Do not get off at Exit 28 in Connecticut).  Turn right onto Lincoln Avenue and proceed approximately one mile to Anderson Hill Road (2nd traffic light).  Turn right onto Anderson Hill Road.  The campus is on the left, just after intersection at Lincoln Avenue







From Connecticut, via I-95:
Take I-95 south then take I-287 West to Exit 9N (Hutchinson River Parkway).  Take Hutchinson River Parkway North to Exit 28, Lincoln Avenue.  Turn left onto Lincoln Avenue and proceed approximately one mile to Anderson Hill Road (2nd traffic light).  Turn right onto Anderson Hill Road.  The campus is immediately on the left.


By Train:

Metro North Schedule Information:
Phone:	(800) METRO-INFO 			(212) 532-4900
www.mta.info/mnr

The White Plains train station maintains a more frequent schedule. Trains from White Plains and Port Chester both end up at Grand Central Station

The last train out of White Plains: 1:14 am (Weekdays and Weekends)
The last train out of Port Chester: 12:58 am (Weekdays and Weekends)


From New York City via rail from Grand Central Station, take the Harlem line/Metro North to White Plains.  Board the Anderson Hill Road bus No. 12 or take a taxi to campus. 

Alternatively, take the New Haven Line/Metro North to Port Chester and take a taxi to campus.

By Bus:

Bus/Westchester: (914) 682-2020
www.beelinebus.com 

Take the No. 12 bus northbound from White Plains or southbound from Yorktown, Mount Kisco, or Armonk. Buses leave approximately once every hour during normal business hours on Weekdays and the schedule varies on weekends
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