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The Performing Arts Center, SUNY Purchase



The Recital Hall
Technical Packet




The Performing Arts Center is a full service performance facility.  The Center maintains a central inventory of equipment for most theatrical and concert needs.  Due to the nature of the facility as a four Theater complex we do not publish inventory lists.  To ensure that the needs of your production are met we request that you communicate your requirements to us as soon as possible, so that we can make the appropriate allocations.  You will find, listed by department, the general types of equipment that we carry.  For further information please feel free to contact the Production Office.

Vectorworks and PDF files of the theater’s ground plan and section, as well as lineset schedule, are available by request. 

For further inquiries about space or equipment availability, please contact the Director of Production at (914) 251-6266 or megan.corkrum@purchase.edu 


The Performing Arts Center's address is

Mailing:
Performing Arts Center,
Purchase College 
ATTN: Production Office
735 Anderson Hill Rd.		
            Purchase, NY  10577

For Shipping to loading docks:
	Please contact the Director of Production for specific instructions (914) 251-6266 






For visiting wireless access: 
Log in: Purchase Guest
Password: (Please Ask Production Staff Member)


THE RECITAL HALL STAGING:
Loading Dock Access:

The Recital Hall has one loading dock, accessed through Parking Lot West 2.  It is truck level and can handle one 53’ tractor trailer at a time.  Dock is available for loading and unloading only.  Short-term and overnight parking for trucks is available by prior arrangement in Parking Lot West 2.


Stage Deck, Stage Lifts, Flooring:

The perimeter area of the stage is floored with a masonite layering.  The stage deck are within the shell features a Stagelam phenolic resin surface.  Due to the nature of this material, lagging and screwing into the floor are prohibtted.  
The Recital Hall is equipped with a full stage lift downstage of the proscenium. Normally the lift acts as an extended apron, however it can accommodate pit orchestras and additional auditorium seating.  For additional seating, the lift can be lowered and an aesthetic wall installed.  For loading in/out and adjusting orchestra pit levels, the lift can operate independently, but must remain stationary during performances.
The Recital Hall has a Harlequin dance floor.  There is enough flooring to cover the playing depth of the theater upstage of the proscenium.  The floor is a black and grey reversible floor. A white Marley floor is available with previous arrangements 

The Center does NOT have a forklift. You will need to rent one if needed

Rigging: 

The theater is equipped with a single purchase counterweight system.  Arbor capacity is 1200 lbs. above batten weight.  The length of each batten is 60'.  There are 4' batten extensions in limited availability.  There are 63 linesets available for variable use in this theater.  Our current lineset schedule is available upon request.  The house curtain is green and a guillotine type, operated from the deck stage right.  There is a center split, but it does not travel.


Labor:

The stagehands at the Performing Arts Center are professional, freelance, union stagehands and wardrobe personnel. We abide by many standard union labor rules. For shows traveling with a “Yellow-Card" we are under the jurisdiction of the New York City and Westchester IATSE Local 1. If you are unfamiliar with the area please contact the Production Office and we will help you arrange your labor through the local Business Office.



General Equipment:

Each theater is equipped with a variety of A-frame ladders and a personnel lift.

The Performing Arts Center owns orchestra chairs, bass stools, music stands and lights for orchestra use.  There are 4'x8' risers in heights of 8", 16" and 24".  We do not own choral risers.  The Recital Hall also houses an acoustical concert shell which is in the onstage position in its standard location. It can be moved off stage by prior arrangement.  It has a variety of possible configurations depending on orchestra size.

The Performing Arts Center maintains a wide assortment of concert quality Steinway pianos which are available by prior arrangement.  Please be advised that THE PERFORMING ARTS CENTER DOES NOT ALLOW TAPE OR ADHESIVES OF ANY KIND ON ANY OF THE PIANOS OR PREPARED PIANO. THERE ARE NO EXCEPTIONS TO THIS POLICY AND WILL BE STRICLTLY ENFORCED.

The PERFORMING ARTS CENTER has a Steinway-trained house piano tuner, contact the Production Office in advance to arrange tunings, standbys and to discuss associated fees. 

The house maintains a lecture package including a lectern, chairs, tables with appropriate skirting, and a front projection movie screen; available by prior request. This theater does not have any projectors

Dressing Rooms:

Dressing rooms for this theater are located one floor below stage level, accessible via stairs stage right and stage left and freight elevator located on stage left.  All have makeup mirrors and lights, with tables and chairs.  There are restroom facilities and showers located in each dressing room.  Rooms break down as follows:

2 chorus rooms		10 people each.
2 chorus rooms		12 people each.
5 private rooms		2 people each.

Laundry:

There are shared laundry facilities located in an adjacent section of the building which must be reserved for use in advance of load-in.  We can supply washing, drying and ironing facilities.  Portable steamers are available through prior arrangement.









Seating Capacity:

Orchestra	476
Boxes	  40
	516

Pit rows	84
Total:	600


Special Effects:

Any special or pyrotechnic effects must be approved by the production office prior to load in.  All necessary and appropriate certificates must be presented upon arrival.

Wireless Coverage:

There is Wi-Fi available on the stage, wings, house, dressing rooms, and the lobby. 
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For visiting wireless access: 
Log in: Purchase Guest
Password: (Please Ask Production Staff Member)



The Recital Hall Dimensions:

Loading Doors:			9'-9"h x 7'-9"w		2.97m x 2.36m
Dock Height:			  	2'-4"				.71m
Control Booth to Plaster Line:	78'-0"				23.77m
FOH Rail to Plaster Line		61' -0"				18.59m
Proscenium Width:			44'-8.5"			13.63m
Proscenium Height: 			30'-0"				9.14m
Total Playing Depth:			61'-0"				18.59m
	(Apron and Lift incld.)
Stage Depth:				43'-11"				13.39m
	(Plaster line to back wall)
Stage Lift Depth at Centerline	9'-9"				2.97m
Apron Depth at Centerline:		8'-0"				2.44m
Stage Left Wing:      			26'-6"				8.08m
Stage Right Wing:			26'-9"				8.15m
Grid Height:	73'-6"		22.40m
High Steel:	80'-6"		24.54m
Batten Working Height:	4'-2"		1.27m
Batten Working Weight:		1200 lbs.			544.3kg
Batten Length:				60'-0"				18.29m
Batten Extension:			4'-0"				1.22m
Masking Opening:			40'-0"				10.97m
Projection Bay:			42'-10"w x 36'-6" d		13.06m x 11.12m


The Recital Hall Drapery Inventory:
Main Curtain	1	34’w x 40’h		10.36m x 12.19m
Black Legs	10	13'w x 35'h		3.96m x 10.67m
Black Borders	5	60'w x 12'h		18.29m x 3.66
Blackout Drops	2	60'w x 35'h		18.29m x 10.67m
Half-Travelers	2	34'w x 35'h		10.36m x 10.67m
Black Scrim	1	65'w x 35'h		19.81m x 12.19m
Natural Bounce	1	65'w x 40'h		19.81m x 12.19m
Front Projection	1	62’w x 30h		18.89m x 9.14m
Dark Rear Projection	1		36’w x 25’h			10.97m x 7.62m










The Recital Hall Electrical Information:


Control Console: 

The Recital Hall is equipped with an ETC Ion 1000, 2x10 Fader Wing, (2) 19” Flat Screen Monitors.  An ETC Net3 RVI with 2 flat screen monitors available. An iPad with Remote App is available on request as the remote for this console. The control booth is located at the rear of Orchestra.  

Company Power:

There is one 400 amps per leg, three phase, 208v disconnect with Camlock tails Ground & Neutral reversed available USR or USL at the mid-rail (parallel).  

In addition, there are three 400A, 208v company switches available in the dimmer room. These four disconnects draw from the same power that feeds the theater’s dimming system. The combined load on the company switches plus the house system cannot exceed 1200 amps/phase.  These disconnects are equipped with cam-lock connectors which are NOT ground & neutral reversed. 

House Dimmers and Circuiting.

The Recital Hall contains a dimmer per circuit system.  There are 338 ETC Sensor dimmers distributed to 2p&g stage circuits as follows:

	Circuits	Cap.	Dimmers	Cap.
	1-308	20 A	1-308	2.4 Kw
	501-530	50 A	309-338	6.0 Kw

House Lights:

House lights are dimmable from the control booth, and from downstage left and downstage right.  House lights may also be controlled through the control console, or any touring console with DMX protocol.

House Hang:

There is a permanent Front of House hang. Overhead are two (2) linesets hung with strip lights without color, predominantly used for worklight and general illumination. These strip lights can be struck as needed. 







Additional Lighting Inventory:

The Performing Arts Center maintains a large inventory of ETC, Altman and other various instruments which is available to the user. Rental charges may apply. Due to the constant rotation of our inventory among our four theaters, we do not list fixtures quantities. Lighting equipment can be requested by completing an “Electrics Request Form”. Below is a list of a selection of fixture types in the PAC Inventory. For further information please contact the PAC Lighting Supervisor or the Production Department (914)251-6262

	Focusing Units
	


Frame Size

	ETC Source Four 5o @575w
	14"x14"

	ETC Source Four 10o @575w
	12"x12"

	ETC Source Four 19o @575w
	6.25"x6.25"

	ETC Source Four 26o @575w
	6.25"x6.25"

	ETC Source Four 36o @575w
	6.25"x6.25"

	ETC Source Four 50o @575w
	6.25"x6.25"

	
	

	Wash Units
	Frames Size

	PAR 64, 1Kw
	10"x10"

	ETC S4 PAR, 750w
	7.5"x7.5"

	8" Fresnel, 1Kw
	10"x10"

	6" Fresnel, 750w
	7.5"x7.5"

	3" Fresnel, 300w
	3.75"x3.75"

	Mini-ten, 1Kw
	8.75"x5.5"

	14" Scoop, T-3, 1Kw
	14"x14"

	Birdie, 150w
	2.75"x2.75"

	GAM Stick-up, 150w
	N.F.

	
	

	

CYC and Border Lights
	

Frames Size

	FAR-CYC, T-3, 4 CKT, 4 light, 1K per CKT, Top/Bottom
	15"x18"

	 ALT T-3, 3 CKT, 6 light, 1K per CKT (Length 4'6")
	8.5"x12.75"

	KLG T-3, 3 CKT, 9 light, 1K per CKT  (Length 6'-9")
	8.5"x8.5"

	KLG T-3, 4 CKT, 8 light, 1K per CKT (Length 6')
	8.5"x8.5"

	KLG T-3 4 CKT 12 light, 1.5K per CKT (length 8')
	7.25"x7.75"





The Recital Hall Audio Information:

Auditorium Amplification:

The Recital Hall has a three channel house speaker system.  

The center cluster is a bi-amplified three-way system containing an EAW MK5164 full-range cabinet, and an EAW SB180 subwoofer flown above the proscenium.  

The left and right stereo cabinets consist of a pair of EAW FR-122 two-way speakers, mounted 12feet above the deck, in the lighting alcove, on brackets that can be swung out of sight when not needed.  

Power for the center cluster is provided by a Carver PM 1.5 amplifier.  Power for the left and right speakers are provided by a 250 watt per channel Carver PM 175 amplifier.

The house console is a Yamaha QL5 digital mixing console.  In addition to the console, the house system is also equipped with a Denon DN-C635 CD player and Tascam 302 dual cassette deck. The console, and associated electronics, are located in the control booth at the rear center of the house. This theater is also equipped with a computer dedicated to audio with a variety of software including Show Cue System, Stage Research SFX, Yamaha Studio editor, Shure wireless workbench, Wavelab 7, Reaper, Dante Virtual Sound Card, etc. All software and firmware is kept to the most current version.

The main house microphone snake has 37 channels, and the main box is located on the proscenium wall back stage right.  Additional single and double microphone input plates are located throughout the theater.  Some input plates on stage are paralleled to the house snake box. There are six audio tie lines running from the theater’s patch bay to a central patch point for the facility that can be used to cross-connect audio from various spaces within the facility.

Communication:

The Recital Hall is equipped with a single channel Clear Com system which is accessible from virtually all points within the theater. 

Additional Audio Equipment:
The Performing Arts Center maintains an extensive inventory of playback equipment, microphones, speakers, amplifiers, signal processing equipment, additional intercom equipment, cables, and accessories. Due to the constant rotation of our inventory among our theaters, we are unable to publish equipment lists. Please reach out to the production department 914-251-6266 regarding the specific needs of your production.

Recordings:
The Recital Hall is acoustically adaptable for recordings. Traps in the stage floor allow passage for microphone snakes to connect with the recording room located one level below the stage, adjacent to the dressing rooms.  We do not supply recording equipment or microphone snakes and a minimum of 75’-100' of cable is required for a recording snake.


Performing Arts Center Contact List:

Megan Corkrum		        (914) 251-6266
Director of Production		megan.corkrum@Purchase.edu

Peter Specce,			(914) 251-6221
Asst. Director of Production		Peter.Specce@Purchase.edu

Justin Herminghouse		(914) 251-6240
Production Technology Manager		Justin.Herminghouse@Purchase.edu

Bennett Marrow			(914) 251-6219
Production Coordinator		Bennett.Marrow@Purchase.edu

Rental Booking Manager		(914) 251-6232
Box Office – Sales/Ticket Purchases		(914) 251-6200
Box Office – Manager		(914) 251-6212

Performing Arts Center Website:		www.artscenter.org
Site contains venue information and e-mail links to most of the center's staff.

DINING
[bookmark: _Hlk217146680]On-Campus Dining hours will change during school breaks
Hours Subject to Change (and quite often do change, especially around holidays) without notice.

Campus Center North/ The Hub			Starbucks 
On Purchase campus				On Purchase Campus
Mon – Fri  7:30am – 12:00am			Located in Fort Awesome
Sat – 10:00am – 1:00am			On Lincoln Ave
Sun – 10:00am- 12:00am			(914) 251-6988
					Mon-Fri 7:30am-11pm
				Sat&Sun 10am-11pm

Enstein Bagels 			 
On Purchase campus	
Located 			
Mon – Fri  7:30am – 3:00pm			
Sat & Sun – Closed	

[bookmark: _Hlk217146623]






HSSospitals & Medical Info: 

White Plains Hospital				Rye Walk-in Medical Center
41 East Post Road					150 Purchase Street
White Plains, NY 10601				Rye, NY 10580 
(914) 681-0600					(914) 967-3266
www.wphospital.org 					M-F 8am-7pm
Sat 9am-2:00pm
Sun 10am-2:00pm

Stop & Shop Pharmacy				Greenwich Hospital
154 Westchester Avenue				5 Perryridge Road
White Plains, NY 10604				Greenwich, CT 06830
914-997-1530		203-863-3000
Mon-Fri: 8am-8am 		www.greenhosp.org
Sat: 9am-5pm
Sun: 9am-3pm



Directions to Purchase College, SUNY Performing Arts Center:


Location Access via:
	Parking Lot West 1
	Underpass in between 
Parking Lots West 1 and West 2
	Parking Lot West 2

	· The Concert Hall “A” Loading Dock
· PepsiCo Theater “B” Loading Dock
	· Main Lobby
· Box office
· Administrative offices
· ADA Elevator
· The Repertory Theater “D” *
Loading Area and Elevator
	· Recital Hall “C”  Loading Dock
· Paint Deck 
  (Concert Hall Alternate Loading Dock)
· ALL Overnight Parking
    (With Prior Approval)


* The Repertory Theater (“D”) does not have a dedicated Loading Dock. Loading is done on street level in the underpass, which has direct access to the stage lift and freight elevator. The Repertory Theater Stage Lift runs from the street level to stage level.

By Car:

From New York City, Southern Westchester, and Long Island:
Take the Hutchinson River Parkway, north to Exit 28, Lincoln Avenue.  Turn left onto Lincoln Avenue and proceed approximately one mile to Anderson Hill Road (2nd traffic light).  Turn right onto Anderson Hill Road.  The campus is immediately on the left.

From Rockland County and Northern New Jersey (via the Tappan Zee Bridge):
Take I-287 (Cross Westchester Expressway) to exit 8E.  Shortly after first traffic light, bear left onto Anderson Hill Road.  Proceed approximately 2.5 miles.  The campus is on the left, just after intersection at Lincoln Avenue.

From Northern Westchester:
Take I-684 south to Exit 2 (Route 120), drive over the bridge and turn right onto Route 120 South (Purchase Street).  Follow Route 120 south, 3.2 miles to Anderson Hill Road (1st traffic light) and turn left.  Take Anderson Hill Road to 2nd traffic light.  The campus is on the left, just after intersection at Lincoln Avenue.

From Connecticut, via the Merritt Parkway (which becomes the Hutchinson River Parkway in New York State):
Proceed south to the New York Exit 28, Lincoln Avenue (Note: Do not get off at Exit 28 in Connecticut).  Turn right onto Lincoln Avenue and proceed approximately one mile to Anderson Hill Road (2nd traffic light).  Turn right onto Anderson Hill Road.  The campus is on the left, just after intersection at Lincoln Avenue







From Connecticut, via I-95:
Take I-95 south then take I-287 West to Exit 9N (Hutchinson River Parkway).  Take Hutchinson River Parkway North to Exit 28, Lincoln Avenue.  Turn left onto Lincoln Avenue and proceed approximately one mile to Anderson Hill Road (2nd traffic light).  Turn right onto Anderson Hill Road.  The campus is immediately on the left.


By Train:

Metro North Schedule Information:
Phone:	(800) METRO-INFO 			(212) 532-4900
www.mta.info/mnr

The White Plains train station maintains a more frequent schedule. Trains from White Plains and Port Chester both end up at Grand Central Station

The last train out of White Plains: 1:14 am (Weekdays and Weekends)
The last train out of Port Chester: 12:58 am (Weekdays and Weekends)


From New York City via rail from Grand Central Station, take the Harlem line/Metro North to White Plains.  Board the Anderson Hill Road bus No. 12 or take a taxi to campus. 

Alternatively, take the New Haven Line/Metro North to Port Chester and take a taxi to campus.

By Bus:

Bus/Westchester: (914) 682-2020
www.beelinebus.com 

Take the No. 12 bus northbound from White Plains or southbound from Yorktown, Mount Kisco, or Armonk. Buses leave approximately once every hour during normal business hours on Weekdays and the schedule varies on weekends
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